**毛纺助剂wool auxiliaries**

**倍捻油 HD-W9905**

**Twisting oil HD-W9905**

**概述:**

本品为矿物油与表面活性剂复配物。适用于多股和单股合成纤维的络筒油剂，因含有特种活性物，在温度发生变化性，不会发生粘度变化。

**Summary:**

This product is a mixture of mineral oil and surfactant. Suitable for multi-unit and single-strand synthetic fiber winding oils, contain special active substance, temperature changes, and the viscosity change will not happen.

**理化性状:**

外观:乳白色液体 电离性:非离子

PH值:5-7

**Physicochemical properties:**

Appearance: Milky white liquid

The ionization: Non-ionic

P H value: 5-7

**产品特性:**

1、可有效降低纤维与金属间的摩擦系数，防止静电产生;

2、无粉尘产生;

3、适用于快速运行的设备;

4、生物降解性好。

**Product Features:**

1,Can effectively reduce the friction coefficient between the fiber and metal to prevent electrostatic generation;2, No dust;

3, Applicable to the rapid operation of the equipment;4 And has good biodegradation.

**使用方法:**

适用于络筒机、加捻机、倍捻机对合成纤维、棉、粘胶、羊毛等纤维的直接加油:

1.用作短纤纱倍捻时用量为:0.3-1%;

2.用作合成纤维的络筒油，用量为1.5-4%(用量取决于纤维种类)。

**Directions for Use:**

Suitable for winding, twisting machine, twisting machine for synthetic fiber, cotton, viscose, wool fiber direct, come on:

1. The amount of time used as a staple yarn twisting is as follows: 0.3-1%

2. The coning oil used in synthetic fibre, the amount of 1.5-4% (the amount depends on the type of fiber).